Scott Le

lesc@sheridancollege.ca

2022-03-04

This document outlines the network infrastructure and the playbooks used to configure the network.

Software Defined Networks

Lab 2



Table of Contents

[Executive Summary 2](#_Toc97839815)

[Network Topology 3](#_Toc97839816)

[Playbooks 4](#_Toc97839817)

[Inventory File 4](#_Toc97839818)

[Host\_vars 5](#_Toc97839819)

[getPAFacts.yml 5](#_Toc97839820)

[getCiscoFacts.yml 7](#_Toc97839821)

[setPA.yml 8](#_Toc97839822)

[setCisco.yml 10](#_Toc97839823)

[Appendix 11](#_Toc97839824)

# Executive Summary

Ansible is an open-source software tool that is used for powerful automation which includes application deployment, cloud provisioning and configuration management. Ansible works by using two types of nodes, a control node which is a host that runs Ansible and managed nodes, devices that are being managed by the control node.

The goal is to focus on the configuration management of Ansible which we will be using to configure Palo Alto Firewalls and a Cisco Router. Through Ansible we will configure the Palo Alto firewalls to have a hostname, DNS server, NTP servers, external and internal zones and an HTTPS policy. We will be also using Ansible to quickly gather facts about the managed devices on our network.

Finally we will describe the topology of the network, our Ansible inventory file, how to execute each playbook and how each playbook works.

# Network Topology

Referring to Figure 1, the image contains our network topology. Inside our network we have two Palo Alto Firewalls, which will be connected on the VMNET10 network. This network will contain the HA link between our two PA firewalls. The PA firewalls will also be connected to the internet to have internet access. Both PA firewalls will be connected to the core router in our topology. The core router will be connected to the rest of our private network. The firewalls will prevent unauthorized access to our private network. All managed devices will be connected on VMNET0 to our control node. The control node will be running Ubuntu/Ansible.




Figure 1: Network Topology

# Playbooks

Ansible playbooks are a blueprint of automation tasks, actions that can be executed with no human or limited involvement needed. Playbooks can be executed on groups or single individual devices, these together make up an Ansible Inventory file. This section will be going through the playbooks that are run against our topology and the inventory that consists of devices inside this network.

## Inventory File

Referring to Fig 2, we have our inventory file which consists of all the devices used in this network. For the router devices in the network, we decided to have subdivided the groups into the parent group Routers and the children group Cisco. We also divide the firewalls the same way, where Firewalls is the parent group and Palo is the children group.

#Inventory file that includes our cisco router, and two PA fws

#Inventory allows for expansion, routers is the parent group to cisco and cisco group contains the router1 host

#Palo parent group houses all the PA FWs used in this topology

[all:vars]

ansible\_user=admin

ansible\_password=admin

[routers:children]

cisco

[cisco]

router1 ansible\_host=172.18.0.7

[cisco:vars]

ansible\_user=admin

ansible\_network\_os=ios

ansible\_connection=network\_cli

[firewalls:children]

palo

[palo]

PA-fw1 ansible\_hosts=172.18.0.8

PA-fw2 ansible\_hosts=172.18.0.9

Figure 2: Host/Inventory File

## Host\_vars

Under our host\_vars folder we have two yaml files for each Palo Alto firewall. Referring to Figure 3 and 4 we have these yaml files that contain parameters that are needed to be provided to “provider”. Provider is a dictionary that is used to make a connection each firewall. The playbooks used will pull these parameters from these yaml files and set them as variables for the provider module.

#YML file for FW1 that includes the variables needed to be provided to provider for PAN-OS connectivity

#Instead of username / password we could provide a API key as well

---

ip\_address: '172.18.0.8'

username: admin

password: admin

Figure 3: PA-FW1.yml

#YML file for FW1 that includes the variables needed to be provided to provider for PAN-OS connectivity

#Instead of username / password we could provide a API key as well

---

ip\_address: '172.18.0.9'

username: admin

password: admin

Figure 4: PA-FW2.yml

## getPAFacts.yml

The first playbook we will examine is getPAFacts.yml. Referring to figure 5, we use the panos collections paloaltonetworks.panos. This collection must be referenced because this is the Ansible collection of modules that are used to automate configuration and operation tasks on Palo Alto firewalls.

The target hosts is “palo” which is our two PA firewalls. This playbook requires connection details for the device to be specified. The variables needed for the connection details are ip\_address, username and password. These variables are defined under the host\_vars folder with each individual yaml file storing the variable values.

The panos\_facts module is used to collect fact information from the Palo Alto firewall, here gather and display facts such as, hostname, serial number of node, model number, PAN-OS version, firewall uptime, number of active sessions and if High-Availability is enabled.

This playbook is used to gather quick facts about the firewall to create a quick audit report.

#Playbook to grab facts from the FW, it will gather facts related to the hostname, serial #, model, PAN-OS version, firewall uptime, HA and the number

# of active sessions

---

- name: Grab Palo Alto facts

  hosts: palo

  connection: local

  collections:

    - paloaltonetworks.panos

#Refer to setPA.yml comments for explaination

  vars:

    device:

      ip\_address: '{{ ip\_address }}'

      username: '{{ username }}'

      password: '{{ password }}'

#Using these tasks we grab facts about the FWs to quickly create an audit report

  tasks:

    - name: Get facts

      panos\_facts:

        provider: '{{device}}'

    - name: Display hostname

      debug:

        msg: "Hostname: {{ansible\_net\_hostname}}"

    - name: Display Serial number of the local node

      debug:

        msg: "Serial number of local node {{ansible\_net\_serial }}"

    - name: Display model, PAN-OS version

      debug:

        msg: "Model: {{ ansible\_facts['net\_model'] }}, version: {{ ansible\_facts['net\_version'] }}"

    - name: Display firewall up time

      debug:

        msg: "Up time: {{ansible\_net\_uptime}}"

    - name: Is High availablity enabled?

      debug:

        msg: "High availablity: {{ansible\_net\_ha\_enabled}}"

    - name: Display number of active sessions firewall

      debug:

        msg: "Current active sessions: {{ansible\_net\_session\_usage}}"

Figure 5: getPAFacts.yml

## getCiscoFacts.yml

This playbook is used to grab quick facts about the Cisco router on the network. The target managed node is router1 which is just a single node under the group cisco. The module used in this playbook is cisco.ios.ios\_facts. Cisco.ios.ios\_facts is used to gather facts about the hostname, serial number, model number, operating system and the management interface. Facts related to the provider are specified inside the inventory file. Referring to figure 2 we specify the connection details, such as username/password and connection type.

#Playbook used to grab quick facts about the router in the network

#Playbook displays the hostname, serial #,  model #, OS, and the management interface

---

  - name: Gather information about Cisco Router

    hosts: router1

    tasks:

      - name: Display hostname

        debug:

          msg: "Hostname: {{ansible\_net\_hostname}}"

      - name: Display serial number and model number

        debug:

          msg: "Serial number of device: {{ansible\_net\_serialnum}}, Model number: {{ansible\_net\_model}}"

      - name: Display Operating system

        debug:

          msg: "Operating system: {{ansible\_net\_version}} "

      - name: Display Management Interface

        debug:

          msg: "GigabitEthernet1: IP address: {{ansible\_net\_interfaces.GigabitEthernet1.ipv4[0].address}}, Subnet mask: /{{ ansible\_net\_interfaces.GigabitEthernet1.ipv4[0].subnet}}"

Figure 6: getCiscoFacts.yml

## setPA.yml

setPA.yml is a playbook used to set configurations on both Palo Alto firewalls. Similar to getPAFacts.yml the targeted hosts are the group palo which contains both PA firewalls.

The modules used in this playbook is panos\_mgtconfig, panos\_zone, panos\_security\_rule and panos\_commit.

Panos\_mgtconfig is used to configure the hostname, dns server, NTP servers and the IPs for Panorama primary and secondary. All of the parameters used for panos\_mgtconfig in this playbook require them to be in string, hence why all variables are in quotations marks. The module panos\_zone is used to configure security zones on PAN-OS firewall, this module needs to be run before the panos\_security\_rule because the zones must be created for the security policy to reference. Panos\_security\_rule module is used to create security rule policies on the PAN-OS firewall, this module requires the security rule name to always be specified. Finally panos\_commit is used to commit the running config of the firewall to the startup config.

#Playbook used to set configurations on both firewalls

---

- name: Set Palo alto configurations

  hosts: palo

#palo is the group variable which houses both fws

  connection: local

# panos collections

  collections:

    - paloaltonetworks.panos

# variables used to pass to the provider module, will pull the values of these inside the host\_vars folder

  vars:

    device:

      ip\_address: '{{ ip\_address }}'

      username: ' {{ username }} '

      password: ' {{ password }} '

  tasks:

    - name: Set hostname, dns servers, NTP servers, panorama primary/secondary

      panos\_mgtconfig:

        provider: '{{ device }} '

# inventory\_hostname will set the hostname to the variable specified inside the inventory file.

        hostname: "{{ inventory\_hostname }}"

        dns\_server\_primary: "1.1.1.1"

        dns\_server\_secondary: "1.1.1.2"

        panorama\_primary: "1.1.1.3"

        panorama\_secondary: "1.1.1.4"

        ntp\_server\_primary: "1.1.1.5"

        ntp\_server\_secondary: "1.1.1.6"

#Zones must be configured first but creating the policy because the policy references zones, if zones aren't created policy will return an error

#Tasks are made to create the internal and external zones

    - name: Configure internal zone

      panos\_zone:

        provider: '{{ device }} '

        zone: 'internal'

        mode: 'layer3'

    - name: Configure external zone

      panos\_zone:

        provider: '{{ device }} '

        zone: 'external'

        mode: 'layer3'

#Task is to allow access for https access from source 172.18.0.1 to any destination

    - name: Set https policy on firewall

      panos\_security\_rule:

        provider: '{{ device }} '

        rule\_name: 'Allow https'

        description: 'Allows https'

        source\_zone: ['internal']

        destination\_zone: ['external']

        source\_ip: ['172.18.0.1']

        source\_user: ['any']

        destination\_ip: ['any']

        category: ['any']

        application: ['any']

        service: ['service-https']

        hip\_profiles: ['any']

        action: 'allow'

# This task is used to commit the changes onto the firewall, alternatively I believe you can commit the changes yourself or have the changes be returned before commiting

    - name: Commit config on firewall

      panos\_commit:

        provider: '{{ device }} '

Figure 7: setPA.yml

## setCisco.yml

The last playbook used in this lab is setCisco.yml. Similar to getCiscoFacts.yml we set the targeted hosts to router1. The modules used to configure the Cisco router is ciso.ios.ios\_hostname, cisco.ios.ios\_banner and cisco.ios.ios\_ntp.

#This playbook is used to configure cisco router used on the topology

#Playbook covers basic modules because our focus was on the firewalls

  - name: Set Cisco configurations

    hosts: router1

    tasks:

    #This task is used to set the host name for the router using the inventory name inside the inventory file

      - name: set hostname

        cisco.ios.ios\_hostname:

          config:

            hostname: “{{ inventory\_hostname }}”

          state: merged

    #Task is used to set the login banner

      - name: Set login banner

        cisco.ios.ios\_banner:

          banner: login

          text: |

            S144 – Lab 2 Ansible

            Cisco Router

          state: present

    #Task is used to set the NTP server to google 8.8.8.8

      - name: Set NTP

        cisco.ios.ios\_ntp:

          server: 8.8.8.8

          logging: false

          state: present

Figure 8: setCisco.yml

# Appendix

root@M-SL:/mnt/c/Users/scott/Documents/Lab2-Ansible# ansible-playbook getPAFacts.yml -i hosts

PLAY [Grab Palo Alto facts] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TASK [Gathering Facts] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [PA-fw1]

ok: [PA-fw2]

TASK [Get facts] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [PA-fw2]

ok: [PA-fw1]

TASK [Display hostname] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [PA-fw1] => {

    "msg": "Hostname: PA-fw1"

}

ok: [PA-fw2] => {

    "msg": "Hostname: PA-fw2"

}

TASK [Display Serial number of the local node] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [PA-fw1] => {

    "msg": "Serial number of local node unknown"

}

ok: [PA-fw2] => {

    "msg": "Serial number of local node unknown"

}

TASK [Display model, PAN-OS version] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [PA-fw1] => {

    "msg": "Model: PA-VM, version: 9.0.1"

}

ok: [PA-fw2] => {

    "msg": "Model: PA-VM, version: 9.0.1"

}

TASK [Display firewall up time] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [PA-fw1] => {

    "msg": "Up time: 0 days, 2:36:54"

}

ok: [PA-fw2] => {

    "msg": "Up time: 0 days, 2:36:59"

}

TASK [Is High availablity enabled?] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [PA-fw1] => {

    "msg": "High availablity: False"

}

ok: [PA-fw2] => {

    "msg": "High availablity: False"

}

TASK [Display number of active sessions firewall] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [PA-fw1] => {

    "msg": "Current active sessions: 0"

}

ok: [PA-fw2] => {

    "msg": "Current active sessions: 0"

}

PLAY RECAP \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PA-fw1                     : ok=8    changed=0    unreachable=0    failed=0    skipped=0    rescued=0    ignored=0

PA-fw2                     : ok=8    changed=0    unreachable=0    failed=0    skipped=0    rescued=0    ignored=0

root@M-SL:/mnt/c/Users/scott/Documents/Lab2-Ansible#

getPAFacts.yml output

root@M-SL:/mnt/c/Users/scott/Documents/Lab2-Ansible# ansible-playbook setPA.yml -i hosts

PLAY [Set Palo alto configurations] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TASK [Gathering Facts] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [PA-fw2]

ok: [PA-fw1]

TASK [Set hostname, dns servers, NTP servers, panorama primary/secondary] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

changed: [PA-fw1]

changed: [PA-fw2]

TASK [Configure internal zone] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [PA-fw1]

ok: [PA-fw2]

TASK [Configure external zone] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [PA-fw2]

ok: [PA-fw1]

TASK [Set https policy on firewall] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [PA-fw1]

ok: [PA-fw2]

TASK [Commit config on firewall] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

[DEPRECATION WARNING]: This module is deprecated; use panos\_commit\_firewall, panos\_commit\_panorama, panos\_commit\_push. This feature will be removed from paloaltonetworks.panos in version 3.0.0. Deprecation warnings can be disabled by

setting deprecation\_warnings=False in ansible.cfg.

changed: [PA-fw2]

changed: [PA-fw1]

PLAY RECAP \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PA-fw1                     : ok=6    changed=2    unreachable=0    failed=0    skipped=0    rescued=0    ignored=0

PA-fw2                     : ok=6    changed=2    unreachable=0    failed=0    skipped=0    rescued=0    ignored=0

setPA.yml output

root@M-SL:/mnt/c/Users/scott/Documents/Lab2-Ansible# ansible-playbook setCisco.yml -i hosts

PLAY [Set Cisco configurations] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TASK [Gathering Facts] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

[WARNING]: Ignoring timeout(10) for ansible.legacy.ios\_facts

ok: [router1]

TASK [set hostname] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [router1]

TASK [Set login banner] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [router1]

TASK [Set NTP] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

[DEPRECATION WARNING]: cisco.ios.ios\_ntp has been deprecated. See the plugin documentation for more details. This feature will be removed from cisco.ios in a release after 2024-01-01. Deprecation warnings can be disabled by setting

deprecation\_warnings=False in ansible.cfg.

ok: [router1]

PLAY RECAP \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

router1                    : ok=4    changed=0    unreachable=0    failed=0    skipped=0    rescued=0    ignored=0

setCisco.yml output

root@M-SL:/mnt/c/Users/scott/Documents/Lab2-Ansible# ansible-playbook getCiscoFacts.yml -i hosts

PLAY [Gather information about Cisco Router] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TASK [Gathering Facts] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

[WARNING]: Ignoring timeout(10) for ansible.legacy.ios\_facts

ok: [router1]

TASK [Display hostname] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [router1] => {

    "msg": "Hostname: router1"

}

TASK [Display serial number and model number] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [router1] => {

    "msg": "Serial number of device: 904MYBCUQ6F, Model number: CSR1000V"

}

TASK [Display Operating system] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [router1] => {

    "msg": "Operating system: 16.09.07 "

}

TASK [Display Management Interface] \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ok: [router1] => {

    "msg": "GigabitEthernet1: IP address: 172.18.0.7, Subnet mask: /20"

}

PLAY RECAP \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

router1                    : ok=5    changed=0    unreachable=0    failed=0    skipped=0    rescued=0    ignored=0

root@M-SL:/mnt/c/Users/scott/Documents/Lab2-Ansible#

getCiscoFacts.yml output